
           SecureCRT(R) 8.1.4 (Official) -- August 10, 2017

            Copyright (C) 1995-2017 VanDyke Software, Inc.
                        All rights reserved.


Product Overview
----------------

SecureCRT protects your passwords, user accounts, and data, combining
rock-solid terminal emulation with the strong encryption, broad
authentication options, and data integrity of the Secure Shell (SSH)
protocol.

SecureCRT provides versatile solutions for business, network manage-
ment, information security, and development tasks, from accessing 
host-based applications and administering servers to securely 
accessing behind-the-firewall network resources like email, files,
and printers.

SecureCRT supports SSH2, SSH1, Telnet, serial, and Raw on all 
platforms.  On Windows, Telnet/TLS, RLogin, and TAPI are supported.
Authentication methods include password, public key, X.509 
certificate, Kerberos v5 via GSSAPI, and keyboard interactive.  
Ciphers include AES-CTR, AES, Twofish, Blowfish, 3DES, and RC4.

Choose from a wide range of emulations, most with ANSI color.  
Unicode support includes the ability to display character sets from 
multiple languages, support for languages with right-to-left reading 
order, and a character encoding list that includes commonly-used 
encodings as well as all encodings supported by the local system.

SecureCRT features a multi-session tabbed or tiled interface with 
extensive session management and customization features.  Customi-
zation options include toolbars and menus (Windows only), keymaps, 
button bar, and login scripts, as well as fonts, cursors, and color 
schemes.  A dockable session manager provides quick connection to 
sessions.

Named sessions and firewalls let you create individual configurations
that can be used on a session-specific basis.  A personal data folder
provides private and separate storage of sensitive information so that 
other configuration data can be stored on a network drive or in the 
cloud for use on different systems or for sharing with colleagues.  
Other features include auto logon, printing, Emacs mode, and SOCKS 
firewall support.

Routine configuration tasks can be automated using powerful scripting 
capabilities including ActiveX scripting support for VBScript, 
JScript, and PerlScript on Windows, embedded Python support on all 
platforms, and the script recorder.  Securely transfer files using 
Zmodem, Xmodem, Ymodem, or Kermit from an SSH1, SSH2, or TLS session.
Upload files easily by dragging and dropping them onto an SFTP tab or 
session window.  A built-in TFTP server provides additional flexi-
bility for transferring files.

Save steps with the close integration of SecureCRT and the SecureFX(R)
file transfer client, which share sessions and settings that let you
run SFTP, FTP, SCP, and FTP/TLS file transfer sessions without
reentering passwords.

SecureCRT includes a 30-day try-before-you-buy evaluation license for
the fully functional application and access to VanDyke Software(R)
technical support.


Contents
--------

   1. New for SecureCRT 8.1
   2. Enhancement Requests, Updates, and Questions
   3. Encryption Export
   4. Upgrades
   5. Product History
   6. SecureCRT Features
   7. Reporting Bugs
   8. Contact Information


1. New For SecureCRT 8.1
------------------------

SecureCRT 8.1 updates the UI on the Mac and Linux platforms with new 
toolbar icons and tab groups, which allow you to easily compare the 
output of two sessions, group related sessions, and switch easily 
between groups.  New productivity enhancements include a hex view, 
new Command window options to send commands to tab groups or visible 
sessions, and the ability to add keywords using the right-click 
menu.  Mac and Linux versions have improved smart card (PIV/CAC) 
support.

Here are some of the new features in SecureCRT 8.1:

Tab groups for Mac and Linux
  Get more done in less time using tab groups. Switch easily between 
  sessions organized in tabs.  Or create a temporary tab group so 
  you can work in one tab while monitoring command output from 
  another tab.

UI enhancements (Mac and Linux)
  SecureCRT for Mac has a new GUI and main toolbar.  Mac and Linux 
  versions have new toolbar icons in the Session Manager and 
  Connect dialog.  Linux makes local shell connections easier with 
  a new toolbar icon.

Enhanced serial support
  A hex view helps to debug serial communication.  When configuring 
  serial sessions only, valid COM ports are shown in the Session 
  Options dialog.

Command window enhancement
  The Command window can now send commands to selected tab groups 
  or visible sessions.
 
Keyword highlighting improvement
  Quickly add keywords to the keyword highlighting list – simply 
  select a word in a session, right-click, and choose “Add 
  keyword…”.

Multi-tab actions (Windows only)
  Select multiple tabs and use the right-click menu to perform the 
  following operations: Send to New Tab Group, Send to New Window, 
  Disconnect, Close, and Lock.

Encryption enhancements

  Enhanced smart card support: On Mac and Linux, select a specific 
  certificate on the smart card (PIV/CAC) to be used for public-key 
  authentication.  PKCS #11 certificates are supported.  On all 
  platforms, the username can be pulled directly from the specified 
  certificate.

  New public-key authentication options (Mac and Linux): Certif-
  icates can be used as raw key.  Public keys can be exported in 
  OpenSSH format and from PKCS #11.

  SSH agent (Mac and Linux): X.509v3 keys can be added to the SSH 
  agent. 

Time-saving enhancements
  The Options menu now includes an “Edit Default Session” item so 
  you can quickly change the default session.  The Session 
  Manager and Connect dialog right-click menus now include “Expand 
  All Folders” and “Collapse All Folders”.

Please see the History tab in the SecureCRT About box for the complete
list of new features, changes, and bug fixes.


2. Enhancement Requests, Updates, and Questions
-----------------------------------------------

We want to hear from you.  Let us know what features you would like to
see in future releases of SecureCRT by visiting our website at:

  https://www.vandyke.com/feedback.php

Every VanDyke Software license includes a full year of upgrades and
technical support.  To receive email notification when new releases
of SecureCRT are available, sign up for our SecureCRT mailing list at:

  https://secure.vandyke.com/cgi-bin/subscribe.php?RMF=3

For tips, ideas, and product news, subscribe to VanDyke Software's
"What's New" at:

  https://whatsnew.vandyke.com

Join the online forums to exchange useful tips and ideas with your 
peers and VanDyke developers:

  https://forums.vandyke.com/index.php?RMF=3

Get online video how-tos on the VanDyke Software YouTube Channel:

  http://youtube.com/vandykesoftware

If you have any questions, please visit our website at:

  https://www.vandyke.com/feedback.php

SecureCRT for Windows supports Windows 10, Windows 8.1, Windows
Server 2012 R2, Windows Server 2012, Windows 8, Windows Server 2008
R2, Windows 7, Windows Server 2008, and Windows Vista for x86 and
x64.  SecureCRT for Mac supports Mac OS X 10.12 and 10.11.  SecureCRT
for Linux supports Ubuntu 14.x, 15.x, and 16.x, and Red Hat Enterprise
Linux 7.0 x64.


3. Encryption Export
--------------------

This Software is subject to export control.  The Software may be
transmitted, exported, or re-exported only under applicable export
laws and restrictions and regulations of the United States Bureau of
Industry and Security or foreign agencies or authorities.  By
downloading or using the Software, you are agreeing to comply with
export controls.  For more information see:

  https://www.vandyke.com/download/export.html


4. Upgrades
-----------

Users who purchased SecureCRT on or after October 1, 2015 are
eligible for a free upgrade to SecureCRT 8.1.  All users can evaluate
SecureCRT 8.1 for 30 days free of charge.  For more information on
upgrade eligibility and purchasing upgrades, please visit:

  https://www.vandyke.com/pricing/corporate/upgrades/index.html


5. Product History
------------------

The list of changes made for this release of SecureCRT can be found
in the SecureCRT_History.txt file installed with the program.


6. SecureCRT Features 
---------------------

Support for SSH1 and SSH2 Secure Shell protocols.
  - SSH2 Protocol support:
    - AES-128, AES-192, AES-256, AES-128-CTR, AES-192-CTR, 
      AES-256-CTR, Twofish, Blowfish, 3DES, and RC4 ciphers.
    - RSA, Ed25519, ECDSA (RFC 5656), DSA, and X.509 (Windows) host 
      key support.
    - Multiple ordered authentication methods, ciphers, and MACs.
    - Public Key Assistant makes it easier to upload public keys.
    - Support for GSSAPI secure key exchange.
    - Local port forwarding, X11 forwarding, remote forwarding, and
      dynamic forwarding.
    - OpenSSH Agent forwarding.
    - SHA2, SHA1, UMAC, and MD5 MACs.
    - Public key with support for RSA (up to 16,384 bits), Ed25519, 
      ECDSA (RFC 5656), DSA, X.509 certificate including SmartCards, 
      PKCS #11, PKCS #12 (Windows only), and Kerberos v5 via GSSAPI.  
      Password and keyboard-interactive authentication methods are 
      also supported.
    - SFTP tab creates an SFTP session to an existing SSH session.
    - Passphrase and password caching options.
  - SSH1 Protocol support:
    - Blowfish, DES, 3DES, and RC4 ciphers.
    - RSA, TIS, and password authentication.
    - Local port forwarding, X11 forwarding.

Session Management.
  - Dockable session manager.
  - Named sessions store different preferences for different hosts.
  - Tabbed sessions allow multiple sessions in the same window.
  - Tab groups make it easier to group related sessions.
  - Launch multiple selected sessions in tabs with a single click.
  - Tiling allows multiple sessions to be viewed at once.
  - A session can be logged to a file, including options for logging
    custom data and a option for creating a new log file at midnight.
  - Built-in SSH agent allows keys to be explicitly added or removed.

Configuration & Customization.
  - Easy configuration of basic SSH, port forwarding, remote
    forwarding, and other settings in Session Options dialog.
  - Named firewalls.
  - Personal data folder for separate storage of logon credentials.
  - Dependent session option (jump host).
  - Customizable toolbar and menus (Windows only).
  - User-defined number of savelines (scrollback) up to 128,000.
  - User-configurable number of rows and columns.
  - User-defined foreground, background, and bold colors.
  - User-defined keymaps.
  - User-defined button bar.
  - User-defined word delimiter characters for double-click.
  - Emacs mode maps ALT+<key> to send ESC+<key>.
  - Real-time keyword highlighting.

Advanced Terminal Emulation.
  - Quality VT100, VT102, VT220, Linux console, SCO ANSI, TN3270,
    Wyse 50/60, and ANSI emulations.
  - VT line drawing.
  - Support for bold, underline, and reverse attributes.
  - Double-width and double-height fonts.
  - 80/132 column switching.
  - VT100 and VT220 keyboard emulation.
  - Optional ANSI color.
  - 256-color Xterm.
  - Xterm extensions for mouse support and changing title bar.
  - Multi-byte character set support for Japanese, Korean, and
    Chinese.
  - Unicode support includes the ability to display character sets
    from multiple languages, support for multi-byte character sets,
    right-to-left reading order languages, and an extensive
    character encoding list.
 
Other Features.
  - FIPS 140-2 validated cryptographic library support (Windows 
    only).
  - Variable compression increases performance on slow connections.
  - Simple interface for automating logins.
  - Support for Telnet, Telnet/TLS (Windows only), and RLogin 
    (Windows only) protocols:
    - Telnet supports Negotiate About Window Size (NAWS).
    - Telnet supports Local Flow Control (LFLOW).
  - Serial (COM) device support.
  - Hex view.
  - Integration with SecureFX.
  - Scripting language support for VBScript, JScript, and Perlscript
    (Windows only).
  - Embedded support for Python scripting.
  - Script recorder.
  - Zmodem, Xmodem, Ymodem, and Kermit file transfer (upload and 
    download).
  - Built-in TFTP server.
  - Drag-and-drop file transfer (upload).
  - Auto print, selection, screen, and pass-through 
    printing.
  - Modem dialer support: configure and save modem, country code,
    phone, and redial settings for TAPI sessions (Windows only).
  - SOCKS firewall support with password authentication.
  - Unauthenticated and basic HTTP proxy support.
  - Generic proxy firewall support.
  - Copy and paste, including an "auto copy" option and a "paste on
    middle or right mouse click" option.
  - Command window option provides an editable type-ahead buffer with
    history support and the ability to send text to the active 
    session, all sessions, specified tab groups, and visible sessions. 
    Use "Send characters immediately" mode to stop commands, edit files 
    using vi, send escape sequences, and do tab completion.
  - Support for use from the command line or web browsers (Windows 
    only).
  - Support for standard insertion caret so that it can be tracked
    by screen access technology for the blind.
  - Import/export tool makes it easy to copy settings between 
    systems.


7. Reporting Bugs
-----------------

If you experience something you believe is a bug, please fill out
our online form at:

  https://www.vandyke.com/feedback.php

Please do not assume someone else will report it.  We will try to
resolve reported bugs as quickly as possible.  However, we can't
resolve bugs that are not reported.

Please describe the problem in as much detail as possible. Please
include the following information:

  - Version of SecureCRT (as shown in the About dialog)
  - Operating system and version


8. Contact Information
-----------------------

For information on ordering licenses, please visit the VanDyke
Software website:

  https://www.vandyke.com


All other inquiries should be directed to:

  VanDyke Software, Inc.
  4848 Tramway Ridge Dr. NE
  Suite 101
  Albuquerque, NM 87111
  USA

  Inquiry form: https://www.vandyke.com/feedback.php


VanDyke Software, SecureCRT, and SecureFX are trademarks or registered
trademarks of VanDyke Software, Inc. in the United States and/or other
countries.

All other products and services mentioned are trademarks or registered
trademarks of their respective companies.